IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2015-05-08T12:13:37"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 3.13.0.0 - Alternate UI 2.12.0.0"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "morrena" of Organization (no name given)
  Owner history of Person "morrena" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PathMasterBudget" | object type "PathMasterBudget" | names: "NBS_COBAFlooring_EntMatt_PathMasterBudget:PathMasterBudget:218431" | material: "NBS_Concept" | property sets: COBie

Types
  IFCBUILDINGELEMENTPROXYTYPE "PathMasterBudget" | USERDEFINED | 1 occurrence | material: "NBS_Concept" | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, Pset_CoveringFlooring, COBie

Property sets
  COBie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "n/a" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Charcoal, Grey, Beige, Brown" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Cost effective polypropylene alternative to traditional aluminium entrance matting systems" (IFCTEXT)
    DurationUnit = "n/a" (IFCTEXT)
    ExpectedLife = "7 years* If used in the correct environment for the volume and type of traffic expected over the system." (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Polypropylene carpet strips with aluminium scraping inserts" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "contact@cobaflooring.com" (IFCTEXT)
    Material = "Polypropylene needlepunch carpet with aluminium scraping inserts. Anti-slip latex backing." (IFCTEXT)
    ModelNumber = "PMB" (IFCTEXT)
    ModelReference = "PathMaster Budget" (IFCTEXT)
    Name = "EntranceMatting_COBAFlooring_PathMasterBudget" (IFCTEXT)
    NominalHeight = 13. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_COBAFlooring_EntranceMatting_PathMasterBudget" (IFCTEXT)
    ManufacturerName = "COBA Flooring" (IFCTEXT)
    ManufacturerURL = "www.cobaeurope.com/flooring/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/pnux3tmp" (IFCTEXT)
    NBSDescription = "Entrance matting" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-35-35/420" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cobaeurope.com/entrance-matting-systems/pathmaster-budget-aluminium-matting/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-57-11/426" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Arrangement = "Internally inset in a matwell" (IFCTEXT)
    BaseColour = "Black" (IFCTEXT)
    BaseMaterial = "Anti-slip latex backing" (IFCTEXT)
    CarpetColourOptions = "Charcoal, Grey, Beige, Brown" (IFCTEXT)
    Construction = "Closed" (IFCTEXT)
    IntegralAccessories = "n/a" (IFCTEXT)
    LinkingJoints = "Aluminium" (IFCTEXT)
    MattingHeight = "13 mm" (IFCTEXT)
    Pattern = "Horizontal strips" (IFCTEXT)
    SurfaceInsertOptions = "Charcoal carpet, Grey carpet, Beige carpet, Brown carpet" (IFCTEXT)
    SurfaceInsertWidth = "n/a" (IFCTEXT)
    TrafficType = "Pedestrian, wheel chairs, pushchairs and trolleys" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Polypropylene carpet strips with aluminium scraping inserts" (IFCTEXT)
    FireRating = "EN 13501 Euro Classification Ef1" (IFCTEXT)
    FlammabilityRating = "Class E" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_CoveringFlooring | properties | on 1 type object
    HasAntiStaticSurface = FALSE (IFCBOOLEAN)
    HasNonSkidSurface = TRUE (IFCBOOLEAN)