IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2015-08-06T11:15:01"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 3.13.0.0 - Alternate UI 2.12.0.0"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "morrena" of Organization (no name given)
  Owner history of Person "morrena" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Plan A Aluminium Entrance Matting" | object type "Plan A Aluminium Entrance Matting" | names: "NBS_COBAFlooring_EntranceMatting_PlanA:Plan A Aluminium Entrance Matting:219554" | material: materials ("NBS_Concept", "NBS_COBAFlooring_Carpet_PlanA") | property sets: COBie

Types
  IFCBUILDINGELEMENTPROXYTYPE "Plan A Aluminium Entrance Matting" | USERDEFINED | 1 occurrence | material: materials ("NBS_Concept", "NBS_COBAFlooring_Carpet_PlanA") | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, Pset_CoveringFlooring, COBie

Property sets
  COBie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "n/a" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Versatile aluminium entrance matting" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Suitable for heavy-duty use" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales@cobaeurope.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Plan A Aluminium Entrance Matting" (IFCTEXT)
    Name = "EntranceMatting_PlanAAluminiumEntranceMatting_COBAFlooring" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "5 years" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_COBAFlooring_EntranceMatting_PlanAAluminiumEntranceMatting" (IFCTEXT)
    ManufacturerName = "COBA Flooring" (IFCTEXT)
    ManufacturerURL = "www.cobaeurope.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/iwz0nwlr" (IFCTEXT)
    NBSDescription = "Entrance matting" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-35-35/420" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cobaeurope.com/entrance-matting-systems/-/datasheets/plan-a.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-57-11/426" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Arrangement = "Can be internally inset in a matwell or loose laid with ramped edging" (IFCTEXT)
    BaseColour = "Aluminium" (IFCTEXT)
    BaseMaterial = "30% recycled aluminium profiles" (IFCTEXT)
    CarpetColourOptions = "Anthracite, Blue, Brown, Charcoal, Grey" (IFCTEXT)
    Colour = "n/a" (IFCTEXT)
    Construction = "Open" (IFCTEXT)
    Dimensions = "n/a" (IFCTEXT)
    IntegralAccessories = "P456 - Aluminium finishing profile, P457 - PVC expansion strip, P460 - T profile, P461 - Frame profile for recessed wells, P463 - Corner pieces for frame profile" (IFCTEXT)
    LinkingJoints = "Black PVC" (IFCTEXT)
    MattingHeight = "18 mm" (IFCTEXT)
    Pattern = "Horizontal strips" (IFCTEXT)
    SurfaceInsertOptions = "Atrium nylon carpet, Needlepunch PP carpet, PVC, Carpet and PVC" (IFCTEXT)
    SurfaceInsertWidth = "20 mm" (IFCTEXT)
    TrafficType = "Pedestrian, wheel chairs, pushchairs and trolleys" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Carpet or PVC strips in an aluminium frame" (IFCTEXT)
    FireRating = "Cfl-s1" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
  Pset_CoveringFlooring | properties | on 1 type object
    HasAntiStaticSurface = TRUE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)