IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2015-08-06T11:19:25"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 3.13.0.0 - Alternate UI 2.12.0.0"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "morrena" of Organization (no name given)
  Owner history of Person "morrena" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Premier Plus Matting" | object type "Premier Plus Matting" | names: "NBS_COBAFlooring_EntranceMatting_PremierPlusMatting:Premier Plus Matting:219554" | material: materials ("NBS_Concept", "NBS_COBAFlooring_Carpet_PremierPlusMatting") | property sets: COBie

Types
  IFCBUILDINGELEMENTPROXYTYPE "Premier Plus Matting" | USERDEFINED | 1 occurrence | material: materials ("NBS_Concept", "NBS_COBAFlooring_Carpet_PremierPlusMatting") | property sets: NBS_General, NBS_Data, Pset_CoveringCommon, Pset_CoveringFlooring, COBie

Property sets
  COBie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "n/a" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Needlepunch interlinking carpet tiles entrance matting" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Effectively scrapes dirt and wipes moisture, links together to cover all floor sizes, Individual tiles can be moved, cleaned or replaced with ease, flexible and easily cut to shape" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales@cobaeurope.com" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Premier Plus Matting" (IFCTEXT)
    Name = "EntranceMatting_PremierPlusMatting_COBAFlooring" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "450 x 300 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "5 years" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_COBAFlooring_EntranceMatting_PremierPlusMatting" (IFCTEXT)
    ManufacturerName = "COBA Flooring" (IFCTEXT)
    ManufacturerURL = "www.cobaeurope.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/ha2r5fby" (IFCTEXT)
    NBSDescription = "Entrance matting" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-35-35/420" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.cobaeurope.com/entrance-matting-systems/-/datasheets/premier-plus.pdf" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "45-57-11/426" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Arrangement = "Internally inset in a matwell" (IFCTEXT)
    BaseColour = "Black" (IFCTEXT)
    BaseMaterial = "100% recycled PVC" (IFCTEXT)
    CarpetColourOptions = "Charcoal, Grey" (IFCTEXT)
    Colour = "n/a" (IFCTEXT)
    Construction = "n/a" (IFCTEXT)
    Dimensions = "450 x 300 mm" (IFCTEXT)
    IntegralAccessories = "Edge, Female connector - 300 mm, Female connector - 450 mm, Male connector - 300 mm, Male connector - 450 mm" (IFCTEXT)
    LinkingJoints = "n/a" (IFCTEXT)
    MattingHeight = "18 mm" (IFCTEXT)
    Pattern = "Horizontal strips (4 per tile)" (IFCTEXT)
    SurfaceInsertOptions = "Needlepunch PP carpet" (IFCTEXT)
    SurfaceInsertWidth = "n/a" (IFCTEXT)
    TrafficType = "Pedestrian, wheel chairs, pushchairs and trolleys" (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Carpet strips in a PVC frame" (IFCTEXT)
    FireRating = "E(F1)" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
  Pset_CoveringFlooring | properties | on 1 type object
    HasAntiStaticSurface = TRUE (IFCBOOLEAN)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)